RESTORATION OF THE MILLENNIUM GREEN FINGERPOST

[image: A photograph of the fingerpost before restoration.] Before work started on the post
[image: A photograph of the fingerpost with the finial removed.] Finial has been removed

[image: A photogra[ph of the finger post being dismantled.] 
Starting to remove the 1st finger
[image: A photograph of the first finger being removed.] 
Removing the 1st finger
[image: A photograph of the first finger off the post.] 
First finger off the post
[image: A phootgraph of the removal of the broken finger.] 
Removal of the broken finger
[image: A photograph showing that the inner post has rusted onto the collar.]

There should be a gap between the inner post and the collar but it is full of rust
[image: A photograph shoing the last finger being removed.]
 Last finger removed
[image: A photograph of the need to use a gas cutter to remove the remains of the inner post.]
Gas cutting to remove the remains of the inner post
[image: A photograph of what was left behind when all  the fingers had been removed.]
 What was left behind
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